---
layout: page
title: "Yeelight Wifi Bulb"
description: "Instructions how to setup Yeelight Wifi devices within Home Assistant."
date: 2016-10-29
sidebar: true
comments: false
sharing: true
footer: true
logo: yeelight.png
ha_category: Light
ha_release: 0.32
ha_iot_class: "Local Polling"
---

The `yeelight` light platform allows you to control your Yeelight Wifi bulbs with Home Assistant.

### {% linkable_title Example configuration %}

To enable those lights, add the following lines to your `configuration.yaml` file:

```yaml
# Example configuration.yaml entry
light:
  - platform: yeelight
    devices:
      192.168.1.25:
        name: Living Room
        transition: 1000
        use_music_mode: True #(defaults to False)
        save_on_change: False #(defaults to True)
      192.168.1.13:
        name: Front Door
```

Configuration variables:

- **ip** (*Required*): IP(s) of your wifi bulbs
- **name** (*Optional*): A friendly name for the device.
- **transition** (*Optional*, default 350): Smooth transitions over time (in ms).
- **use_music_mode** (*Optional*, default False): Enable music mode.
- **save_on_change** (*Optional*, default True): Saves the bulb state when changed from Home Assistant.

#### {% linkable_title Music mode  %}
Per default the bulb limits the amount of requests per minute to 60, a limitation which can be bypassed by enabling the music mode. In music mode the bulb is commanded to connect back to a socket provided by the component and it tries to keep the connection open, which may not be wanted in all use-cases.

### {% linkable_title Initial setup %}
<p class='note'>
Before trying to control your light through Home Assistant, you have to setup your bulb using Yeelight app. ( [Android](https://play.google.com/store/apps/details?id=com.yeelight.cherry&hl=fr), [IOS](https://itunes.apple.com/us/app/yeelight/id977125608?mt=8) ).
In the bulb property, you have to enable "Developer Mode"  Developer mode may only be available with the latest firmware installed on your bulb.  Firmware can be updated in the application after connecting the bulb.
Determine your bulb IP (using router, software, ping ...)
</p>

<p class='note warning'>
This component is tested to work with the following models. If you have a different model and it is working please let us know.
</p>

- **YLDP01YL**: LED Bulb (White)
- **YLDP02YL**: LED Bulb (Color)
- **YLDP03YL**: LED Bulb (Color) - E26
- **YLDD02YL**: Lightstrip (Color)





