<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<board>
<plain>
<hole x="95.25" y="34.29" drill="4"/>
<hole x="95.25" y="67.31" drill="4"/>
<text>PRG</text>
<text>TX</text>
<text>RX</text>
<text>GND</text>
<text>VCC</text>
<wire x1="62.23" y1="67.31" x2="62.23" y2="34.29" width="0.508" layer="20"/>
<wire x1="62.23" y1="34.29" x2="64.77" y2="29.21" width="0.508" layer="20" curve="43.602819"/>
<wire x1="64.77" y1="29.21" x2="97.79" y2="29.21" width="0.508" layer="20"/>
<wire x1="62.23" y1="67.31" x2="64.77" y2="72.39" width="0.508" layer="20" curve="-43.602819"/>
<wire x1="64.77" y1="72.39" x2="97.79" y2="72.39" width="0.508" layer="20"/>
<wire x1="100.33" y1="34.29" x2="100.33" y2="67.31" width="0.508" layer="20"/>
<wire x1="100.33" y1="67.31" x2="97.79" y2="72.39" width="0.508" layer="20" curve="43.602819"/>
<wire x1="100.33" y1="34.29" x2="97.79" y2="29.21" width="0.508" layer="20" curve="-43.602819"/>
<text>ESP8266 BUTTON</text>
</plain>
<libraries>
<library name="esp8266modules">
<packages>
<package name="ESP12-SMD">
<description>ESP8266 Module 12 SMD pads</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Seeed-OPL-Button">
<packages>
<package name="SW5-2.0-8.8X4.4X4.7MM-90D">
</package>
</packages>
</library>
<library name="Seeed-Connector">
<packages>
<package name="H2-5.0-10.5X8.0MM">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Large - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="esp8266modules" package="ESP12-SMD" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-09435"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-09435"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="SWITCH">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="SW1" library="Seeed-OPL-Button" package="SW5-2.0-8.8X4.4X4.7MM-90D" value="SK-12D01">
<attribute name="MPN" value="SK-12D01"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-09435"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="Seeed-Connector" package="H2-5.0-10.5X8.0MM" value="GREEN-2P-5.0"/>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U2" pad="VCC"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U2" pad="GPIO2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="GND"/>
<contactref element="R2" pad="P$2"/>
<contactref element="RESET" pad="1"/>
<contactref element="U2" pad="GPIO15"/>
<contactref element="SW1" pad="A"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="RESET" pad="3"/>
<contactref element="U2" pad="RESET"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="CH_PD"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="TXD0"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="RXD0"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="GPIO0"/>
<contactref element="SW1" pad="COM"/>
<contactref element="R3" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
